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Abstrak
Karbon aktif sekam padi (RHAC) dihasilkan dan digunakan untuk menghilangkan warna pewarna organik dan efluen kilang kelapa sawit (POME) melalui proses penjerapan. Sekam padi dikarbonisasi dan diaktifkan menggunakan kalium hidroksida (KOH) dan natrium hidroksida (NaOH) untuk menghasilkan karbon aktif. Sifat karbon aktif (AC) dikaji melalui analisis permukaan dan morfologi. Penjanaan semula bahan penjerap dengan proses penjerapan/penyaherapan menunjukkan bahawa AC dapat dijana semula hingga lima kitaran sementara masih memberikan maksimum 67.26% kapasiti penjerapan pada regenerasi pertama dan serendah 2.72% kapasiti penjerapan pada regenerasi kelima. RHAC juga digunakan untuk perawatan POME untuk penyahwarnaan dan pengurangan jumlah karbon organik (TOC) dan permintaan oksigen kimia (COD). Kajian ini menunjukkan bahawa RHAC berpotensi digunakan sebagai bahan penjerap untuk menghilangkan pelbagai jenis cas positif bahan terjerap dan POME dari larutan berair.

Kata kunci:  karbon aktif, sekam padi, penjerapan, karbonisasi, efluen kilang kelapa sawit
 
 Abstract
Rice husk activated carbon (RHAC) is produced and used to remove the color of organic dyes and palm oil mill effluents (POME) through an adsorption process. Rice husk is carbonized and activated using potassium hydroxide (KOH) and sodium hydroxide (NaOH) to produce activated carbon. The properties of activated carbon (AC) were studied through surface and morphological analysis. Adsorbent regeneration by adsorption/absorption process showed that AC could be regenerated for up to five cycles while still providing a maximum of 67.26% adsorption capacity on the first regeneration and as low as 2.72% adsorption capacity on the fifth regeneration. RHAC is also used for POME treatment for discoloration and reduction of total organic carbon (TOC) and chemical oxygen demand (COD). This study shows that RHAC has the potential to be used as an adsorbent to remove various types of positive charge adsorbate and POME from aqueous solutions.
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